SOLID COUNTERS 

Construction from 18mm melamine with 25mm tops & 3mm Hi-Impact, 
heat-sealed edging. 
Glass counters are constructed as above using 6mm float glass.

CHOOSE FROM BASIC COLOURS OF WHITE, GREY OR CREAM 
WITH TRIM COLOUR OF RED, BLUE, GREEN OR BURGANDY.

OTHER COLOURS AVAILABLE AT EXTRA CHARGE.

WOODGRAIN Effect in various types of timbers also available at extra charge.

GLASS FRONT & TOP COUNTER 

MEASUREMENTS W x H x D

1000 x 900 x 600		
1200 x 900 x 600				
1800 x 900 x 600		

OPTIONAL GLASS OR SOLID DOORS AVAILABLE FOR GLASS FRONTED COUNTERS.					
Please phone for prices & availability.		

Delivery will be quoted depending on size & location.

NB All counters are made to order so please allow for construction & delivery.

***Just call 01206 576872 for more details.***